Code 122 refers to the transmission of the longitudinal drawer and in particular to activation

**24S6.** The activation of this alarm stops the equipment, it disables the power transformer

connection relay. All movements are disabled, the angle of tilt display flashes and shows the

alarm code while the remaining displays switch off.

